#include<stdio.h>

#include<fcntl.h>

#include<termios.h>

#include<string.h>

#include<wiringPi.h>

#include<stdlib.h>

char value;

char \*Serialport ="/dev/ttyS0";

char number[] ="6476741649";

void setupgsm()

{

int f, count;

char buf[10];

serialport.begin(9600);

serialport.println("gsm module intilization through serialport");

delay(38000);

}

void gsmsms()

{

serialport.println("AT");

serialport.println("AT+CMGH=1");

serialport.print("AT+CMGS=");

serialport.print(number);

delay(500);

serialport.print("object\_status");

delay(1500);

}